Home > Specifications > General Specifications

### General Specifications

Printer Type | Laser
Print Method | Electrophotographic Laser Printer
Memory Capacity | Standard | 32 MB
LCD (liquid crystal display) | (LJ2655DN) 16 characters × 1 line
Power Source | 220 - 240 V AC 50/60 Hz
Power Consumption (Average) | Peak *1 | Approximately 1080 W
Printing *1 | Approximately 537 W at 25 °C
Printing (Quiet Mode) *1 | Approximately 331 W at 25 °C
Ready *1 | Approximately 58 W at 25 °C
Sleep *1 | Approximately 5.4 W
Deep Sleep *1 | (LJ2405D/LJ2455D/LJ2605D) Approximately 0.4 W (LJ2655DN) Approximately 0.5 W
Power Off *1 *2 *3 | Approximately 0.06 W
Dimensions |
Weights (with supplies) | 6.8 kg

*1
Measured when the machine is connected to the USB interface.
*2
Measured according to IEC 62301 Edition 2.0.
*3
Power consumption varies slightly depending on the usage environment.

Noise Level | Sound Pressure | Printing | LpAm = 50 dB (A)
Ready | LpAm = 30 dB (A)
Printing (Quiet Mode) | LpAm = 45 dB (A)
Sound Power | Printing *1 | LWAd = 6.52 B (A)
Ready *1 | LWAd = 4.55 B (A)
Printing (Quiet Mode) | LWAd = 6.06 B (A)
Temperature | Operating | 10 to 32 °C *2
Storage | 0 to 40 °C
Humidity | Operating | 20 to 80% (without condensation)
Storage | 10 to 90% (without condensation)

*1
Measured in accordance with the method described in RAL-UZ171.
*2
To ensure the high print quality, the maximum ambient temperature we recommend is 32 °C. The maximum ambient temperature to safely use this machine is 35 °C.

Related Information
  - Specifications
  - Settings Table

Go to top of page