# Bonjour
Device Management > Configuration > Network > Bonjour

Configure settings related to Bonjour (Rendezvous).
Some items are for reference only and cannot be changed.

Note

- Bonjour (formerly known as Rendezvous) was launched upon the release of Mac OS X 10.4.
- Settings configured here relate to the following interfaces:
  Ethernet and wireless LAN.
- Settings on this page can be changed by the following administrators and users:
  - Network Administrator
  - Login users
    User authentication is enabled on the device and users are permitted to make changes to administrator's setting items.

### Bonjour

Specify whether Bonjour for the device's interface boards is active or inactive.

#### IPv4

Specify whether or not to enable Bonjour when using the machine on an IPv4 network.

#### IPv6

Specify whether or not to enable Bonjour when using the machine on an IPv6 network.

## Ethernet/Wireless LAN/Ethernet + Wireless LAN

Ethernet, Wireless LAN, or Ethernet + Wireless LAN appears depending on the interface board installed.

### Local Hostname

Displays the Bonjour host name.
This indicates the host name of the network interface board or wireless LAN board, to which ".local" is appended.

Note

- The Bonjour name may consist of the IPv4 host name followed by a hyphen and number, for example: IPHostName-2.local. If two or more devices with the same host name are connected to the same LAN, a sequence number is appended to the host name.

## Details

These settings are common to the network interface board and wireless LAN board.

### Computer Name

Enter a name to identify the device using Bonjour, using up to 63 characters.
The default is the manufacturer's name followed by the device model.

### Location

Enter the device location, using up to 32 characters. This item is linked to Location on the Device Management - Configuration - Device Settings - System page.

## Print Order Priority

### DIPRINT, LPR, IPP

Enter the priority for each protocol type, between 0 and 99. The lower the value, the higher the priority.
The default is 10 for DIPRINT, 20 for LPR, and 30 for IPP.

## Buttons

### Refresh

Click to update the currently displayed information.

Note

- Before making the settings, click Refresh to obtain the machine's current status.

### OK

Click to apply the settings.

### Cancel

Click to cancel the settings.

##