# Network Application
Network Settings > Network Application

Use this tab to configure the network print and mDNS settings.

## Scanner Send Setting

Select the scanning functions that you want to use.

## Network Print Setting

Select the printing protocols that you want to use.
If you select RAW, you must also specify the port number. You can specify a value between 1024 and 65535, but not 5222, 5353, 6006, 28900, 29102, 49999, or 53550.

## mDNS Setting

### mDNS

Make the setting for mDNS (multicast DNS). If you select Active, specify the printer name.

### Printer Name

Enter the printer name, using up to 32 alphanumeric characters.

## Buttons

### Refresh

Click to update the currently displayed information.

Note

- Before making the settings, click Refresh to obtain the machine's current status.

### Please enter Administrator Password.

Enter the administrator password.

Note

- If you enter a wrong password or leave the text box blank, the settings on this tab will not be applied when you click OK.

### OK

Click to apply the settings.

### Cancel

Click to cancel the settings.

##