///////////////////////////////////////////////////////////////////////////

    - StarPRNT Intelligence -
        FirmwareInfo file                                     26/1/2015

///////////////////////////////////////////////////////////////////////////
* This file shows printer firmware version which is required by StarPRNT 
  Intelligence Version 2.3 and limitation with using old firmware.

[For TSP650 Users]
  StarPRNT Intelligence Version 2.3 does not support TSP650.
  Use StarPRNT Intelligence Version 1.5 as this supports TSP650.

[Required printer firmware version]
  The printer firmware version which is required by StarPRNT Intelligence 2.3 
  is as follows.

    - SP500    (V4.0 or later)
    - SP700    (V3.0 or later)
    - FVP10    (V1.2 or later)
    - TSP650II (V1.0 or later)
    - TSP700II (V3.0 or later)
    - TSP800II (V1.4 or later)
    - TUP500   (V4.0 or later)
    - TUP900   (V5.0 or later)

[Required printer firmware version for Bluetooth interface]
  To use Bluetooth interface, the following printer firmware version is required.

    - TSP650II (V1.0 or later)
    - TSP700II (V5.0 or later)
    - TSP800II (V2.0 or later)
    - SP742    (V4.0 or later)
    - FVP10    (V2.0 or later)

  To use [Printer Utility - Printer Settings - Data Timeout], 
  the following printer firmware version is required.

    - TSP650II (V2.0 or later)
    - TSP700II (V5.0 or later)
    - TSP800II (V2.0 or later)
    - SP742    (V4.0 or later)
    - FVP10    (V2.0 or later)

  To use [Printer Utility - Printer Settings - Hardware Connection Check (Data Timeout)], 
  the following printer firmware version and interface board firmware version are required.
  To confirm your interface board version, please use Star Bluetooth Utility.

    - TSP650II (V2.1 or later, IFBD-HB05)
    - TSP700II (V5.1 or later, IFBD-HB05)
    - TSP800II (V2.1 or later, IFBD-HB05)
    - SP742    (V4.1 or later, IFBD-HB06)
    - FVP10    (V2.0 or later, IFBD-BB05)


[limitation with using old firmware]
1. TUP900
    2-1. In the case of using USB Printer Class
      Before you use the printer, turn off the Dip Switch 1-6 to change 
      USB Mode to the Mode 1.
      Printer driver and utility will not work correctly without this setting, 

2. TSP700II
    2-1. In the case of using firmware version V1.2 or older.
      Printer driver will not work correctly in the case of using firmware version V1.2 or older.
      If you are using version V1.2 or older, please contact store you bought the printer from.

3. Printer Driver
    3-1. 'Data Treatment Recovery From Error'
      'Clear Data By Document Unit' function do not work following version.
      Even select that function, printer works as 'Store Data'.

      - SP700    (older than V3.0)
      - FVP10    (older than V1.2)
      - TSP700II (older than V3.0)
      - TSP800II (older than V1.2)
      - TUP500   (older than V4.0)
      - TUP900   (older than V5.0)

4. [Printer Utility - Printer Settings]
  4-1. 
    'Reset Defaults' function do not work following versions.

    - TSP700II (older than V3.0)
    - TSP800II (older than V1.2)
    - TUP500   (older than V3.0)
    - TUP900   (older than V5.0)

  4-2. 'Printer Performance'
    'Print Speed' do not work following versions.

     - TSP800II (older than V1.3)

5. [Printer Utility - Logo Store]
   [Printer Utility - Troubleshooting]
  5-1. 
    If the 'Printable Area' is set to '80mm' or '72mm' in 
    [Printer Utility - Printer Settings], test print may not work 
    correctly.
