Certificate

Overview
  This page allows you to configure a certificate and the corresponding secret key for this Device.
  This Device supports two certification methods. A self-signed certificate and a certificate that is issued by a CA (Certificate Authority).
Use self-signed certificate
  This Device issues its own certificate.
  It is easier to use this type of certificate with functions rather than using a certificate from a CA.
Use a certificate from a CA.
  There are two ways to create a certificate from a CA. Method 1: using a CSR (Certificate Signing Request) from this Device. Method 2: The CA to create a certificate and a secret key.
  Please use this if you already have a CA or would like to use a certificate from an outside trusted CA.
  NOTE:
  Some functions are disabled depending on the status of the certificate configuration.
  The functions are grayed and unlinked.
Certificate List
  Display the list of certificates which are installed on this Device
View
  The contents of the certificate are displayed.
Delete
  Delete the certificate and secret key from this Device
Export
  This Device exports the certificate and secret key.
Create Self-Signed Certificate
  This Device creates a self-signed certificate and installs it by itself.
  It is easier to use this type of certificate with functions rather then using a certificate from a CA.
  There are now two choices to select with the Public Key Algorithim and Digest Algorithim.
  When you connect to a device which does not support the higher security, please lower the security settings .
Create CSR
  This Device creates a CSR to be issued with a certificate from a CA.
  After the CA issues a certificate, install the certificate in the page "Install Certificate."
  You can select a Public Key Algorithm and Digest Algorithm security levels, to create a Self-Signed Certificate.
Install Certificate
  This Device installs a certificate from the CA.
  Only a certificate issued with this Device CSR can be installed.
  To use SSL/TLS communication with this Device, the certificate from the CA needs to be installed at the computer communicating with the Device.
  NOTE:
  This function is enabled after creating a CSR.
Import Certificate and Private Key
  This Device imports the certificate and Private key.