Active Directory Authentication

Overview
  This page allows you to modify the Active Directory Authentication parameters.
Storage Fax RX Data
  This setting determines whether users need to authenticate with Active Directory when printing received faxes. If this setting is On, Fax RX data is temporarily stored and only printed after the user has authenticated.
Active Directory Server Address
  This field determines the host name or IP address of the Active Directory server. (Eg. ad.example.net -or- 192.0.0.1) If you are using the DNS name of the Active Directory server you must use the FQDN (Fully Qualified Domain Name) such as ad.example.net.
Protocol & Authentication Method
  Select the Protocol & Authentication Method you wish to use to connect and authenticate to the Active Directory server.
  connect via LDAP and authenticate with kerberos
  connect via CIFS(SMB) and authenticate with kerberos
  connect via CIFS(SMB) and authenticate with NTLMv2
Get Mail Address
  This setting determines whether to acquire the user's E-Mail Address. If this setting is On, the user's E-mail Address will be used in the from fileld when using the Scan to E-mail function.
LDAP Server Port
  Enter the port number to connect the Active Directory server via LDAP. The Default LDAP port number is 389.
LDAP Search Root
  Enter the DN (Distinguished Name) of the location to acquire the user's E-Mail Address. (Eg. dc=example,c=us) The Search Root must be less than 256 bytes and can only use UTF8 characters.