Welcome to use TOSHIBA SIDM Printer
You can get more information from our site: http://www.toshiba-tec.com/
You also can find driver installation in manual for detail. 

This CD-ROM includes the printer drivers for the following OS: Windows 2000, Windows XP, Windows 7 32bits, windows 7 64bits, Windows 8.
In the driver folder, there are two executable files:
安装驱动(32位系统).exe is to install driver in 32-bit OS while 安装驱动(64位系统).exe is for 64-bit OS.


~~~~~~~~Windows 7 Driver installation~~~~~~~~
1. Turn on the PC and log on as a user with administrative privileges
2. Double-click the TOSHIBA Driver Installer icon and start the installation
3. When the User Account Control message pop out, click [Yes]. 
4. Select the printer model to be installed from the list then click [Install] button once enabled.
Note: The installation process automatically removes and uninstalls all the existing TOSHIBA Serial Impact Dot Matrix drivers in the PC
5. Disconnect the printer from the PC or turn off the printer when prompted by the dialog. Click [OK] button to proceed or [Cancel] to end the installation process.
6. When installing by USB or parallel interface, connect the printer then turn it on as instructed in the dialog. Otherwise, the driver will be installed using COM1. Click [OK] button to proceed or [Cancel] to end installation.
7. When "Windows Security" dialog appears, check [Always trust software from "Toshiba Tec Singapore Pte Ltd"] then click [Install].
8. A dialog appears to indicate successful installation using the port specified.


~~~~~~~~Windows 8 Driver installation~~~~~~~~
1. Turn on the PC and log on as a user with administrative privileges
2. Double-click the TOSHIBA Driver Installer icon and start the installation
3. When the User Account Control message pop out, click [Yes]. 
4. Select the printer model to be installed from the list then click [Install] button once enabled.
Note: The installation process automatically removes and uninstalls all the existing TOSHIBA Serial Impact Dot Matrix drivers in the PC
5. Disconnect the printer from the PC or turn off the printer when prompted by the dialog. Click [OK] button to proceed or [Cancel] to end the installation process.
6. Delete all TOSHIBA TS-8xx0F printer from "Devices and Printers" folder when prompted.
7. When all printer icons for TOSHIBA TS-8xx0F have been removed, click the [OK] button in the installer's dialog to continue.
8. When installing by USB or parallel interface, connect the printer then turn it on as instructed in the dialog. Otherwise, the driver will be installed using COM1. Click [OK] button to proceed or [Cancel] to end installation.
9. When "Windows Security" dialog appears, check [Always trust software from "Toshiba Tec Singapore Pte Ltd" then click [Install].
10. A dialog appears to indicate successful installation using the port specified.



~~~~~~~~Windows XP Driver installation~~~~~~~~
1. Turn on the PC and log on as a user with administrative privileges
2. Double-click the TOSHIBA Driver Installer icon and start the installation
3. Select the printer model to be installed from the list then click [Install] button once enabled.
Note: The installation process automatically removes and uninstalls all the existing TOSHIBA Serial Impact Dot Matrix drivers in the PC
4. Disconnect the printer from the PC or turn off the printer when prompted by the dialog. Click [OK] button to proceed or [Cancel] to end the installation process.
5. When installing by USB or parallel interface, connect the printer then turn it on as instructed in the dialog. Otherwise, the driver will be installed using COM1. Click [OK] button to proceed or [Cancel] to end installation.
6. When "Software Installation" diag appears, select [Continue Anyway].
7. A dialog appears to indicate successful installation using the port specified.


~~~~~~~~Windows 2000 Driver installation~~~~~~~~
1. Turn on the PC and log on as a user with administrative privileges
2. Double-click the TOSHIBA Driver Installer icon and start the installation
3. Select the printer model to be installed from the list then click [Install] button once enabled.
Note: The installation process automatically removes and uninstalls all the existing TOSHIBA Serial Impact Dot Matrix drivers in the PC
4. Disconnect the printer from the PC or turn off the printer when prompted by the dialog. Click [OK] button to proceed or [Cancel] to end the installation process.
5. When installing by USB or parallel interface, connect the printer then turn it on as instructed in the dialog. Otherwise, the driver will be installed using COM1. Click [OK] button to proceed or [Cancel] to end installation.
6. When "Digital Signature Not Found" diag appears, select [Yes].
7. A dialog appears to indicate successful installation using the port specified.

