Toshiba e-STUDIO Series

	Copyright(c) 2008-2020 Toshiba Tec Corporation, All Rights Reserved.
			 August 20, 2020

This product has the following restrictions and issues.  Please be sure to read this before using.

--------------------------------------------------------------------------------
Installation
--------------------------------------------------------------------------------

When you use Windows Server 2008, install Desktop Experience via Administrative Tools in advance.
(1) Start > Administrative Tools > Server Manager
(2) Click [Add Features].
(3) Select the [Desktop Experience] checkbox and click the [Next] button.
(4) Click the [Install] button.
(5) When installation results are displayed, click the [Close] button.
(6) When you are asked if you want to restart your computer, click the [Yes] button to restart.

--------------------------------------------------------------------------------
e-STUDIO WIA Driver            		Version 4.1.14.0 
--------------------------------------------------------------------------------

This software supports the following models:
- e-STUDIO6550C Series
- e-STUDIO4540C Series
- e-STUDIO6530C Series
- e-STUDIO4520C Series
- e-STUDIO455 Series
- e-STUDIO855 Series
- e-STUDIO456 Series
- e-STUDIO856 Series
- e-STUDIO2550C Series
- e-STUDIO407CS Series
- e-STUDIO527S Series
- e-STUDIO507 Series
- e-STUDIO857 Series
- e-STUDIO6570C Series
- e-STUDIO5005AC Series
- e-STUDIO5008A Series
- e-STUDIO7506AC Series
- e-STUDIO8508A Series
- Loops-LP30_e-STUDIO306LP
- e-STUDIO307LP_Loops-LP301
- e-STUDIO5008LP_Loops-LP50 Series
- e-STUDIO5015AC Series
- e-STUDIO5018A Series
- e-STUDIO7516AC Series
- e-STUDIO8518A Series
- e-STUDIO400AC Series

Issues 
========

1. Notes on Using the WIA Driver
(1) Touch Panel during WIA Connection
- During WIA scan, the operation panel only displays special screens for RemoteScan.
- By pressing the [CANCEL] button on the operation panel, a WIA connection session can be forcibly terminated.
* Buttons other than [CANCEL] are disabled.
* Canceling from the client application or a TopAccess scan job is possible.
* WIA scan connection continues until image transfer to the client PC is finished.  Therefore, it may take several minutes before other operations become available after the scan is completed.
(2) Restrictions on the WIA Driver
- No notification report is transmitted whether WIA scan is completed normally or abnormally.
- When power failure occurs during WIA scan, the job will be lost.  Start all over again.

(3) When using Windows Server 2008, set the startup type for the Windows Image Acquisition (WIA) service to [Automatic] using the management tool beforehand.
 1. Right-click [My Computer].
 2. Select [Manage].
 3. Click [Services and Applications].
 4. Click [Services].
 5. Double-click [Windows Image Acquisition (WIA)].
 6. On the [General] tab, select [Automatic] in the [Startup Type] box.
 7. Click [Apply] and [OK].

(4) When using Windows Server 2008, set the startup type for the PnP-X IP Bus Enumerator service to [Automatic] using the management tool beforehand.
 1. Right-click [My Computer].
 2. Select [Manage].
 3. Click [Services and Applications].
 4. Click [Services].
 5. Double-click [PnP-X IP Bus Enumerator].
 6. On the [General] tab, select [Automatic] in the [Startup Type] box.
 7. Click [Apply] and [OK].

(5) When you use an imaging application to scan a document, configure the following settings before scanning:  When the settings have not been configured, scanned images become black.
 1. Select [Tools] -> [Options] -> [Scan] from the imaging application menu bar.
 2. Click the [Advanced] button.
 3. Check [Native].

(6) When you click the [Cancel] button to cancel scanning of a document using Photoshop or other TWAIN-compliant imaging applications, restart the application to scan the document.

(7) Scanning with resolution lower than the default of the scan profile which was set by the client computer may not be performed.
    In that case, set the default resolution of the scan profile to resolution appropriate for scanning.

(8) When the user authentication and department management functions are enabled, a WIA driver cannot be operated from a computer.
    To operate it, disable these functions.

(9) If you use the e-STUDIO Series on which the user authentication is effective, perform the following procedure before scanning.
 When you use Devices and Printers or Windows Fax and Scan:
 1. In the [New Scan] window, click the [Change] button.
 2. When [Select Device] is displayed, choose the Toshiba MFP and click [Properties] button.
 3. When the department authentication is enabled in the Toshiba MFP, click [Device Settings] tab.
    In another case of authentication, close the Properties dialog box.
 4. Click the [Department Code] button in the Department Code box.
 5. When the User Authentication dialog box is displayed, input the correct department code and click the [OK] button.

When the driver is used from another application, configure similar settings in the Properties dialog box.

--------------------------------------------------------------------------------
Trademarks
--------------------------------------------------------------------------------

- The official name of Windows Vista is Microsoft Windows Vista Operating System.
- The official name of Windows Server 2008 is Microsoft Windows Server 2008 Operating System.
- Microsoft, Windows and the brand names and product names of other Microsoft products are trademarks of Microsoft Corporation in the US and other countries.
- Other company names and product names in this manual are the trademarks of their respective companies.
