[default]
ModuleName=Scan Manager Pro
title=Scan Manager Pro

[error101]
title=Scan Manager Pro
text=Hardware not found

[error102]
title=System configuration problem
text=USB not accessible

[error103]
title=Scan Manager Pro
text=Multiple accesses to Scan Manager are not allowed. Please close one, then reacquire the scanner.

[error104]
title=Scan Manager Pro
text=The scan size was too large. Please change the size.

[error105]
title=Scan Manager Pro
text=The scan size was too large. Please change the size.

[scannername]
9300=OneTouch 9320
9200=OneTouch 9220
9000=OneTouch 9020

DefaultID=9300

[option]
RunMatrix=0 	            // 1: Apply 3x3 Matrix; 0: Not Apply 
DefaultGamma=1.0
PosDefaultGamma=1.0
GrayDefaultGamma=1.0
sValue=1.2      	    // sValue: diagonal line value of 3x3 Matrix; Other elements of 3x3 Matrix is -(sValue-1)/2
DumpLut=0                   // 1: Dump upper LUT to file for debug; 0: No Dump
PositiveApplyColorMatch=0   // (for ScanManager Pro)
NegativeApplyColorMatch=1   // (for ScanManager Pro)
RefColorMatch=1             // 1: Enable Color Matching; 0: Disable 
AdfColorMatch=1             // 1: Enable Color Matching; 0: Disable 
PostiveCutLine=0    	    // 1: Cut Pos uppper boundry; 0: Not Cut (for ScanManager Pro)
PostiveBoundValue=13 	    // Cut Pos uppper boundry when Std<PostiveBoundValue(for ScanManager Pro)
CMatchID=115                // Set A&W Color model ID
NegDoColorConvertionR=0     // 1: Rotate Neg Pattern right 90 degree; 0: Disable(for ScanManager Pro)
UseAgfaCm=1                 // 1: Use Pmx Color Matching; 0: Use A&W Color Matching 
SaveAGCInfoBmp=1  	    // 1: Save Image before send to Color Table; 0: Not Save(for ScanManager Pro)
NegDoColorConvertion=1      // 1: Call A&W NegColorConvertion function; 0: Not call (for ScanManager Pro)
UseAGCCurve=1               // 1: Set A&W analysised R,G,B curves to driver; 0: Not set (for ScanManager Pro)


UseAfCmRef=0 		    // 1: Use Pmx FB color matching when 48bits; 0: Not use (for ScanManager Pro)
UseAfCmPos=0   		    // 1: Use Pmx Pos color matching when 48bits; 0: Not use (for ScanManager Pro)
UseAfCmNeg=0                // 1: Use Pmx Neg color matching when 48bits; 0: Not use (for ScanManager Pro)


CmFileNameRef=LMABQCRF.bmp   
CmFileNameAdf=LMABQCAF.bmp   