////////// Format///////////////////////////////////////////
//----Setup Section--[UmaxSetup]
//DefaultAdapter=Default Adapter ID
//Adapters=Adapter ID List
//----Adapter Section--[Adapter ID]
//Description=Adapter Description which will be shown
//            when installation progresses.
//Driver16=driver name(*.sys:Dos ASPI or *.386:Windows VxD)
//Driver32=driver name(*.mpd, Windows 95 miniport driver),
//         inf file(adapter inf file),
//         install section
//         (If the field is missed, setup programe will not register
//          driver. This design is used for PNP SCSI adapter)
//         option(CHECKEXIST:copy only if des. file does not exist,
//                otherwise, always overwrite.
//DriverNT=driver name(*.sys, Windows NT miniport driver)
//Nots. If driver name(or key) is missed, the driver for
//      the specific adapter will not be installed.
//
//  Modification for VistaScan 3.0:
//
//    All SCSI adapter driver will be installed if they were
//    listed in [UmaxSetup] section
//
//////////////////////////////////////////////////////////////
//////////////////////////////////////////////////////////////

[UmaxSetup]
DefaultAdapter=DMX3191D
Adapters=DMX3191D,AEC671X, AdvanSys39x2, ASPI Compatible

[UDS-IS10]
Description="UMAX SCSI Card: UDS-IS10"
Driver16=vumaxd.386
Driver32=umaxis10.mpd,UNISscsi.inf,Install.UDSIS10
DriverNT=umaxmini.sys

[UDS-IS11]
Description="UMAX SCSI Card: UDS-IS11"
Driver16=umaxis11.386
Driver32=umaxis11.mpd,UNISscsi.inf,Install.UDSIS11
DriverNT=umaxis11.sys

[AVA 1502P]
Description="UMAX SCSI Card: Adaptec AVA 1502P"
Driver16=aspi2pnp.sys
Driver32=umaxis11.mpd,umaxscsi.inf,Install.UDSIS11,CHECKEXIST
AutoSwitch=TRUE


[DMX3191D]
Description="DOMEX SCSI Card"
Driver16=aspi3191.sys
Driver32=dmx3191.mpd,dmx3191.inf,
DriverNT=dmx3191.sys

[AEC671X]
Description="AEC SCSI Card"
Driver16=aspi671x.sys
Driver32=aec671x.mpd,aec671x.inf,
DriverNT=aec671x.sys

[AdvanSys39x2]
Description="AdvanSys SCSI Card"
Driver32=asc.mpd,UNISasc.inf,
DriverNT=..\\disk2\\asc.sys,,,CheckVersion32


[ASPI Compatible]
Description="ASPI Compatible"
