# This file is generated by the Printer Status Monitor.
#
# When the IP address setting of print controller is changed,
# the dialog is often indicated as "No response. Make sure the
# specified IP address is correct."
# If you want to monitor the printer, exit the printer status
# monitor, do the operation from A to D as follows, and start the
# printer status monitor.
#
# A. Check the power of printer whether it is on or not.
# B. When the power is on, check the IP addresses by the following
#    operations.
#    1. For the operation panel, push the printer key and change to
#       the screen for printer mode.
#    2. Make the offline condition by touching the offline key.
#    3. Touch the "MENU" key.
#    4. Touch the "NETWORK SETTINGS".
#    5. Touch the "IP ADDRESS SETTING", and check the IP address.
# C.  If you use LPR software or LPR port on NT, 
#    1. Double-click the icon "My Computer", and double-click the
#       "Printer" icon.
#    2. Right-click the icon of the printer, and select "Properties".
#    3. For the "port to print to" in the "Details" tab (When it is
#       NT, "Print to the following port(s)." in the "Ports".),
#       select the port that is the correct IP address.
# D.  For the "port to print to", when you use LPR software that does
#     not use the IP address, or print by way of a server, describe
#     the correct IP address by editing this file.
#
#
# Syntax:
# IP-Address Printer-Name-Shown-In-The-Explorer
#
#         Printer-Name-Shown-In-The-Explorer : (This must be the name
#         used in "Printers".)
#
# Example:
# 192.168.122.23 SHARP AR-507 PCL6
# 192.168.122.24 SHARP AL-1600 Series PCL6
# 192.168.122.25 SHARP AR-160/200 Series PCL6
# 192.168.122.26 SHARP DM-2000 Series PCL6
# 192.168.122.27 SHARP AR-235 PCL6
# 192.168.122.28 SHARP AR-P350 PCL6
# 192.168.122.29 SHARP AR-M350 PCL6
