Home > Network > Learn to Use Network Management Software and Utilities > Install or Access Network Management Software and Utilities > Access Web Based Management > Set a Logon Password for Web Based Management

### Set a Logon Password for Web Based Management

Related Models:LJ2655DN
We recommend setting a logon password to prevent unauthorized access to Web Based Management.

1. Start your web browser.
2. Type "http://machine's IP address" in your browser's address bar (where "machine's IP address" is the machine's IP address).
   For example: http://192.168.1.2

   - If you are using a Domain Name System or enable a NetBIOS name, you can type another name, such as "SharedPrinter" instead of the IP address.

     - For example:

       http://SharedPrinter

     If you enable a NetBIOS name, you can also use the node name.

     - For example:

       http://brnxxxxxxxxxxxx

     The NetBIOS name can be found in the Network Configuration Report.

   - For Macintosh, access Web Based Management by clicking the machine's icon on the Status Monitor screen.
3. No password is required by default. Type a password if you have set one, and then click .
4. Click Administrator.
5. Type the password you want to use (up to 32 characters).
6. Retype the password in the Confirm New Password box.
7. Click Submit.

In the future, every time you access Web Based Management, type the password in the Login box, and then click .

After configuring the settings, log off by clicking .

If you are not setting a logon password, you can also set a password by clicking the Please configure the password button on the machine's web page.

Related Information
  - Access Web Based Management

Go to top of page