# Paper
Device Management > Configuration > Device Settings > Paper

Use this page to configure settings for paper loaded in paper trays, such as size and type, for each paper tray.

Note

- For the bypass tray, the value set in the Paper Size box applies only when using the printer function.
- Settings on this page can be changed by the following administrators and users:
  - Machine Administrator
  - Login users
    User authentication is enabled on the device and users are permitted to make changes to administrator's setting items.

## Tray Settings

### Select Tray Paper Settings

Use one of the following methods to specify the settings of paper loaded in the input tray.

#### Custom Paper

You can apply the settings of a custom paper that is already registered on the Custom Paper page.

#### Tray Paper Settings

Manually configure the settings of the paper specified for the input tray, using the settings under Tray Paper Settings.

### Recall Custom Paper

If you specify Custom Paper for Select Tray Paper Settings, you must then specify a custom paper in the list to apply its settings. To view the settings of a registered custom paper, click Check Modes.

### Tray Paper Settings

If you specify Tray Paper Settings for Select Tray Paper Settings, you must then specify the following settings manually for the paper loaded in the input tray:

#### Paper Size

In the Paper Size list, select the size of paper loaded in the input tray.
When Custom Size is selected, also select an appropriate option in the Custom Paper Size box.

Note

- Available values depend on machine type and paper tray.

#### Custom Paper Size

Enter the custom paper size when Custom Size is selected.
Enter the length of the paper's short and long edges, in the Horizontal and Vertical boxes respectively, in the units set on the machine (inch or mm).

Note

- Available paper sizes vary depending on the paper tray. For details about setting the paper size, see the operating instructions provided with the machine.
- This appears only for trays on which Custom Size can be set as the paper size.

#### Paper Type

Select the paper type in the box.

Note

- Available options vary depending on machine and paper tray.
- This item appears only for paper trays where users can select paper type.

#### Paper Weight

Select the paper weight from the drop down menu.

Note

- Available values depend on machine type and paper tray.
- This item appears only for paper trays where users can select paper type and weight.
- If you select a paper type other than Plain Paper in the Paper Type list, the paper type - not the paper weight - will be displayed for Input tray on the Status page.
  For example, if you select Plain Paper in the Paper Type list and Thick Paper 1 in the Paper Weight list, Thick Paper 1 will be displayed. However, if you select Recycled Paper in the Paper Type list and Thick Paper 1 in the Paper Weight list, Recycled Paper will be displayed.

#### Apply Auto Paper Select

Select to use the tray when Auto Select is chosen as the paper source.
When On is selected, the tray is automatically selected according to the job settings.
When Off is selected, the tray is not used even if the size and type of paper loaded in the tray matches the job settings. This option can be used to prevent paper loaded in the tray, such as high quality paper and special paper, automatically feeding.

Note

- This item may not appear depending on machine configuration.

#### Apply Duplex

Specify whether to use the tray for duplex printing.
Even if On is selected, the tray may not be suitable for duplex printing, depending on the type and weight of the paper that is loaded in it.

## Low Paper Detection

### Select Threshold for "Almost Out of Paper" Notification

Select a threshold level for the Almost Out of Paper notification on the Status page.

## Buttons

### Refresh

Click to update the currently displayed information.

Note

- Before making the settings, click Refresh to obtain the machine's current status.

### OK

Click to apply the settings.

### Cancel

Click to cancel the settings.

##