# Tray Paper Settings
System Settings > Tray Paper Settings

Use this tab to configure settings for paper loaded in paper trays, such as size and type, for each paper tray.

## Tray 1

### Paper Size

Select AutoDetect or select the size of the paper loaded in the tray from the list.
When Custom Size is selected, specify the size below.

### Unit

Select the units used to enter length in the Horizontal and Vertical boxes, when Custom Size is selected.

### Horizontal/Vertical

Enter the custom paper size when Custom Size is selected.
Enter the length of the paper's short and long edges, in the Horizontal and Vertical boxes respectively, in the units set above (inch or mm).

Note

- Paper sizes that can be detected with AutoDetect are A3 SEF, A4 SEF, A4 LEF, B4 SEF, B5 SEF, B5 LEF, B6 SEF, 11 x 17 SEF, 8 1/2 x 14 SEF, 8 1/2 x 11 SEF, 11 x 8 1/2 LEF, and 10 1/2 x 7 1/4 LEF.
- Available paper sizes vary depending on the paper tray. For details about setting the paper size, see the printer operating instructions.

### Paper Type

In the list, select the paper type.

## Tray 2/Tray 3

Note

- These settings appear only if Tray 2 or Tray 3 is installed.

### Paper Size

Select AutoDetect or select the size of the paper loaded in the tray from the list.
When Custom Size is selected, specify the size below.

### Unit

Select the units used to enter length in the Horizontal and Vertical boxes, when Custom Size is selected.

### Horizontal/Vertical

Enter the custom paper size when Custom Size is selected.
Enter the length of the paper's short and long edges, in the Horizontal and Vertical boxes respectively, in the units set above (inch or mm).

Note

- Paper sizes that can be detected with AutoDetect are A3 SEF, A4 SEF, A4 LEF, B4 SEF, B5 SEF, B5 LEF, B6 SEF, 11 x 17 SEF, 8 1/2 x 14 SEF, 8 1/2 x 11 SEF, 11 x 8 1/2 LEF, and 10 1/2 x 7 1/4 LEF.
- Available paper sizes vary depending on the paper tray. For details about setting the paper size, see the printer operating instructions.

### Paper Type

In the list, select the paper type.

## Bypass Tray

### Paper Size

Select AutoDetect or select the size of the paper loaded in the tray from the list.
When Custom Size is selected, specify the size below.

### Unit

Select the units used to enter length in the Horizontal and Vertical boxes, when Custom Size is selected.

### Horizontal/Vertical

Enter the custom paper size when Custom Size is selected.
Enter the length of the paper's short and long edges, in the Horizontal and Vertical boxes respectively, in the units set above (inch or mm).

Note

- Paper sizes that can be detected with AutoDetect are A3 SEF, A4 SEF, A4 LEF, B4 SEF, B5 SEF, B5 LEF, A5 SEF, A5 LEF, B6 SEF, 11 x 17 SEF, 8 1/2 x 14 SEF, 8 1/2 x 11 SEF, 11 x 8 1/2 LEF, 10 1/2 x 7 1/4 LEF, and 5 1/2 x 8 1/2 SEF.
- Available paper sizes vary depending on the paper tray. For details about setting the paper size, see the printer operating instructions.

### Paper Type

In the list, select the paper type.

## Bypass Tray Setting Priority

When Auto Tray Select is chosen as the paper source in a job, specify whether to give priority to the device's paper settings (such as paper size and type) or to the job's paper settings.

#### System Settings

Jobs are printed using the paper settings configured on the device. If the device's paper settings do not match the paper settings configured for the job, a paper mismatch error will occur.

#### Any Size/Type

Even if the paper settings configured on the device do not match the paper settings configured for the job, a paper mismatch error will not occur and the jobs will be printed from the bypass tray.

#### Any Custom Size/Type

This setting can be applied only if the paper size specified for the job is a custom size. Even if the paper settings do not match the paper settings configured on the device, a paper mismatch error will not occur and the jobs will be printed from the bypass tray.

## Specified Tray

Sets the specified tray.

## Size mismatch detection

When a tray other than Auto Tray Select is chosen as the paper source in a job, specify whether or not to detect the paper size mismatch.
Jobs will be printed from the tray even if the paper size configured for the job does not match the size of the paper loaded in the specified tray. However, when this function detects a paper size mismatch, a paper mismatch error will occur.

## Buttons

### Refresh

Click to update the currently displayed information.

Note

- Before making the settings, click Refresh to obtain the machine's current status.

### Please enter Administrator Password.

Enter the administrator password.

Note

- If you enter a wrong password or leave the text box blank, the settings on this tab will not be applied when you click OK.

### OK

Click to apply the settings.

### Cancel

Click to cancel the settings.

##