# SNMP
Network Settings > SNMP

Use this tab to configure the SNMP settings.

## SNMP

Select whether SNMP is active or inactive for the interface board.

## Trap

### Target Trap

Specify whether or not to notify the managers with trap messages.
If you enable this function, information about errors will be sent to the IP address/host name specified in SNMP Management Host 1 and SNMP Management Host 2.

### SNMP Management Host 1

Enter the IP address or host name of the recipient host, using up to 64 alphanumeric characters (including dashes "-", underscores "_", colons ":", and periods ".").

### SNMP Management Host 2

Enter the IP address or host name of the recipient host, using up to 64 alphanumeric characters (including dashes "-", underscores "_", colons ":", and periods ".").

## Community

### Get Community

Specify the name of the get community, using up to 15 alphanumeric characters. The default name is "public".
The name you specify here is used to retrieve information from the SNMP agent. If the community name is different from that of the hosts, requests from the hosts will not be accepted.

### Trap Community

Specify the name of the trap community, using up to 32 alphanumeric characters. The default name is "public".
The name you specify here is used to receive trap messages sent from the SNMP agent. If the community name is different from that of the hosts, trap messages to the hosts will not be received.

## System

### Location

Enter a text string detailing the machine's location, using up to 64 alphanumeric characters.
The information you enter here appears on the Status tab of the Home page.

### Contact

Enter a text string detailing the contact information, using up to 64 alphanumeric characters.
The information you enter here appears on the Status tab of the Home page.

## Buttons

### Refresh

Click to update the currently displayed information.

Note

- Before making the settings, click Refresh to obtain the machine's current status.

### Please enter Administrator Password.

Enter the administrator password.

Note

- If you enter a wrong password or leave the text box blank, the settings on this tab will not be applied when you click OK.

### OK

Click to apply the settings.

### Cancel

Click to cancel the settings.

##