# Energy Saver Mode
Administrator Tools > Energy Saver Mode

Use this tab to configure the energy saver mode settings.

## Energy Saver Mode

### Energy Saver Mode 1

Specify whether or not to enable energy saver mode 1.
If you select Active, the machine enters energy saver mode 1 when the machine has been idle for about 30 seconds. It takes less time to recover from energy saver mode 1 than from energy saver mode 2, but power consumption is higher in energy saver mode 1 than in energy saver mode 2.

### Energy Saver Mode 2

Depending on the printer you are using, different items to be displayed.

#### Waiting Time (1-60 minutes)

You can select from 1 to 60 minutes for the machine to wait before it enters energy saver mode 2.
Specify a time between 1 and 60 (minutes).
The machine enters energy saver mode 2 after the period of time specified for this setting elapses.

#### Waiting Time (1-240 minutes)

Specify whether or not to enable energy saver mode 2.
If you select Active, specify the waiting time between 1 and 240 (minutes).
The machine enters energy saver mode 2 after the period of time specified for this setting elapses.

### Silent Print Mode

If you execute a print job when energy saver mode 2 is Active, it changes to silent print mode.
When the time set in silent print mode has elapsed, the machine returns to energy saver mode 2.

#### Waiting Time (1-120 seconds)

Specify a time between 1 and 120 (seconds).
If the period of time specified for this setting elapses, the machine enters energy saver mode 2.

## Buttons

### Refresh

Click to update the currently displayed information.

Note

- Before making the settings, click Refresh to obtain the machine's current status.

### Please enter Administrator Password.

Enter the administrator password.

Note

- If you enter a wrong password or leave the text box blank, the settings on this tab will not be applied when you click OK.

### OK

Click to apply the settings.

### Cancel

Click to cancel the settings.

##