# Program/Change E-mail Address Destination
Scan Destination > Program/Change E-mail Address Destination

Use this page to specify e-mail address destination settings.

### ID (Required)

Register the e-mail address destination. Select an ID from 1 to 100.

### Name (Required)

Enter the name of the destination. You can enter up to 16 alphanumeric characters. The name specified here is shown on the screen when you select a scan destination.

### Destination E-mail Address (Required)

Enter the e-mail address destination. You can enter up to 64 alphanumeric characters.

### Notification E-mail Address (Optional)

Enter the e-mail address to send a notification after transmission. You can enter up to 64 alphanumeric characters.

### Subject (Required)

Enter the subject of the e-mail. You can enter up to 64 alphanumeric characters.

### Sender's Name (Optional)

Enter the name of the e-mail sender. You can enter up to 32 alphanumeric characters.

### File Format (Color/Gray Scale)

File format of the scanned file when scanning in color. PDF or JPEG can be selected. PDF supports multiple pages in a document, but JPEG does not.

### File Format (Black & White)

File format of the scanned file when scanning in black and white. PDF or TIFF can be selected. Both formats support multiple pages in a document.

### Scanning Mode

Specify the scanning mode for black and white scanning. Select from color, grayscale, or black and white.

### Original

Select the sides of the original (1- or 2-sided) to scan according to the orientation of the page and binding.

### Scan Size

Select the scanning size for the original from AutoDetect, A3 SEF, B4 SEF, A4 SEF, A4 LEF, B5 SEF, B5 LEF, A5 SEF, A5 LEF, B6 SEF, 11 x 17 SEF, 8 1/2 x 11 SEF, 11 x 8 1/2 LEF, 8 1/2 x 13 SEF, 8 1/2 x 14 SEF, 8 1/2 x 13.4 SEF, 5 1/2 x 8 1/2 SEF, 16K SEF, 16K LEF, 8K SEF, or Custom Size.
If you select Custom Size or AutoDetect, select mm or Inch, and then specify the width and length.

### Resolution

Select the scan resolution from 100 x 100dpi, 150 x 150dpi, 200 x 200dpi, 300 x 300dpi, or 600 x 600dpi.

### Density

Specify the image density by clicking the right or left button.

## Buttons

### Refresh

Click to update the currently displayed information.

Note

- Before making the settings, click Refresh to obtain the machine's current status.

### Please enter Administrator Password.

Enter the administrator password.

Note

- If you enter a wrong password or leave the text box blank, the settings on this tab will not be applied when you click OK.

### OK

Click to apply the settings.

### Cancel

Click to cancel the settings.

##