;  UNISSCSI.INF


[Version]
signature="$Windows 95$"
Class=SCSIAdapter
Provider=%UNISCAN%

[ClassInstall]
Addreg=SCSIReg

[SCSIReg]
HKR,,,0,%SCSIClassName%
HKR,,Intaller,,UNISCAN.DLL
HKR,,Icon,,"1,UNISCAN.DLL"

[Manufacturer]
%UNISCAN%=UNISCAN

[UNISCAN]
%UNISIS10.DevDesc%=Install.UDSIS10, UDSIS10
%UNISIS11.DevDesc%=Install.UDSIS11, UDSIS11

[Install.UDSIS10]
LogConfig = UDSIS10_NoDMA
Copyfiles = MoveMiniPort.UDSIS10
AddReg    = IOS, UDSIS10_RegEntries

[Install.UDSIS11]
LogConfig = UDSIS11_NoDMA
Copyfiles = MoveMiniPort.UDSIS11
AddReg    = IOS, UDSIS11_RegEntries

[UDSIS10_NoDMA]
;ConfigPriority=REBOOT
;ConfigPriority=HARDRECONFIG
ConfigPriority = DESIRED
;IOConfig=280-28F(3ff::),290-29F(3ff::),300-30F(3ff::),310-31F(3ff::),330-33F(3ff::),340-34F(3ff::),348-357(3ff::),350-35F(3ff::)

[UDSIS11_NoDMA]
;ConfigPriority=REBOOT
;ConfigPriority=HARDRECONFIG
ConfigPriority = DESIRED
;IOConfig=220-23F(3ff::),240-25F(3ff::),280-29F(3ff::),2A0-2BF(3ff::),2C0-2DF(3ff::),300-31F(3ff::),320-33F(3ff::),340-35F(3ff::)

[IOS]
HKR,,DevLoader,,*IOS
HKR,,DontLoadIfConflict,,"Y"

[UDSIS10_RegEntries]
HKR,,PortDriver,,UNISIS10.MPD

[UDSIS11_RegEntries]
HKR,,PortDriver,,UNISIS11.MPD

[DestinationDirs]
MoveMiniPort.UDSIS10=12
MoveMiniPort.UDSIS11=12

[SourceDisksFiles]
UNISIS10.MPD=1
UNISIS11.MPD=1

[SourceDisksNames]
1 = %ID1%,,

[MoveMiniPort.UDSIS10]
UNISIS10.MPD

[MoveMiniPort.UDSIS11]
UNISIS11.MPD

[Strings]
SCSIClassName="SCSI Controller"
UNISCAN="UNISCAN Inc."
UNISIS10.DevDesc="UNISCAN IS10 SCSI Card"
UNISIS11.DevDesc="UNISCAN IS11 SCSI Card"
ID1="UNISCAN IS10 SCSI driver for Windows 95"
